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Handheld Data Terminal
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Salute to the classics    Newly upgraded



[image: ]
1. Advantages
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High Performance Computing Platform
Octa-core 64-bit Cortex-A55 processor (up to 2.0 GHz), plus a 200M RISC-V Co-processor make all kinds of massive data processing smoothly.
Android 14.0
Android 14.0 OS, keeps optimizing and upgrading.

Top Class Materials
Cast Aluminium + PC body, with tempered glass provide excellent rigidity + heat dissipation + electromagnetic shielding features. Soft material around the handle offers a comfortable grip.

Industrial-grade Components
Industrial-grade and military-grade components ensure stable operation in harsh environments.

Ultra Long Operating Time
Pistol style hot-swappable battery system makes backup battery more convenient to be restored, so that the operating time is unlimited.( Extra batteries are available.)
High-end UHF RFID Engine
Equipped with self-developed UHF RFID module, it is reputable in the industry for the outstanding reliability and stability and extremely strong multi-tag identification performance.
Outstanding Industrial Design
The idea was inspired by orca, and each single detail has been well refined. The appearance is compact, elegant and balanced, which makes the product eye-catching and impressive.

Excellent Mechanical Protection
Safety drop height 1.6m. IP64 protection grade.
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3. Electrical Parameters
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Android
 
14.0
Octa-core 64-bit Cortex-A55
 
/up to 2.0 GHz
+ a 200M RISC-V Co-processor
G57
 
MC1
4G+
64
G
5.0 inches/ 1280*720
 
/ IPS
 
/ 180°view angl
e
1.1
mm
 
thickness
 
tempered
 
glass
/
 
5-
dot 
touch/ operable
 
with
 
gloves
Pistol style
 
hotswapping
 
batte
ry
 
system
3 
ALPS buttons/ Operating for
ce 2.2N /
Operating life
 
1
 
million cycles
OMRON button
 
/ Operating force 1.27N/
Operating life 10
 
million
 
cycles
7
,000mAh chargeable Ii-polymer
 
battery
Micro 
SIM card
 
slot*1
 
/
 
T
F
 
card
 
slot*1
(Supports up to 256GB Micro SD  card)
USB 3.0 TYPE C (OTG support
ed)
28mm*9mm*3.8mm
Button style
 
/ 10mm diameter
) (
Operating System
CPU
GPU
RAM+ROM
LCD
Touch Screen
Hotswapping Battery
Power/Volume
Scan Trigger
Power
Card Slots
Interface
Speaker Size
Vibration
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Mechanical parameters
Materials                           
Cast
 
Aluminium
 
+
 
PC
Dimensions
                       
 
Body  
167mm*82mm
*130mm
                                         
Grip
    
111mm*38mm*47mm
Weight                               
615g（Battery included）
System
 
Characteristics
) (
Wireless Communications
WIFi
 
Cmu
Bluetooth
LTE
Application
 
Environm
ent
-20℃~+60℃
-30℃~+70℃
5%RH
 
- 95%RH
 
(non -condensing)
 
IP64
1.6m /
 
5.25ft
Operating Temp
 
Storage Temp
Work
 
Humidity
    
Protection Grade
Safety
 
Drop
 
Height
2.4G/5G Dual-Band
 
Bluetooth
 
5.0
Supported
)Data Collections
1D/2D Barcode
Datamatrix/QRCode/PDF417 US Planet/ UK Postal, etc.



UPC/EA SymbolSE955N/Code128/
Code39/Code93/Code11/lnterleaved 2 of 5/
Discrete 2 of 5/Chinese 2 of 5/
Codabar/MSI/ RSS, etc.

UHF RFID
-85dbm
EPC Global UHF Class 1 Gen 2/ ISO 18000-6C 
902~928MHz, 865~868MHz  

0~33dBm

>500tags/s

4dBi circularly polarized antenna

>12m (Tested with lmpinj E41binlay)
US, Canada and other regions
Following U.S. FCC
Europe and other regions following
ETSI EN 302 208
China
Korea
Malaysia

13 megapixels/ automatic focus/ flashlight

Global positioning system
Accessories

Charger &
Data Cable
Sensitivity
Protocol
Frequency
RF Output Power
Peak Inventory Speed
UHF Antenna
Read Distance
Supported Regions
GPS & GLONASS & Beidou
Charging Bay
Hanging Lace
Optional [image: ]
Battery
Camera
2D
1D
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